**Prestan Manikin Chest Assembly Script (1:35)**

Today we will show you how to replace the compression assembly.

We’re going to start by removing the old chest plate. Next, turn the manikin over and pop off the wire cover using a flat edge screwdriver.

If you’re using a monitored manikin, disconnect the clicker from the monitor. Pop out the clicker. Remove the small spring and piston sleeve.

With the new assembly, insert the small spring into the piston sleeve. Insert both into the manikin, ensuring the spring is facing out and the slots are aligned.

Snap the new clicker into place, reconnect the wires, and replace the wire cover.

Turn the manikin back over.

Align the new chest plate with the xiphoid process guide facing the bottom of the manikin.

For best results, press and hold down the chest while tightening the screw. A cordless screwdriver is helpful for this.

Just close the cover and you’re ready to go.